Identification_Information:
  Citation:
    Citation_Information:
      Originator: Michael Baker Jr., Inc.
      Publication_Date: Unknown
      Title: HydroWest
      Geospatial_Data_Presentation_Form: vector digital data
      Online_Linkage: \\CHOLMES-D400\D\CuyahogaWest\ContoursWest\Block_04\Geodatabase\Block04.mdb
  Description:
    Abstract: Hydrography derived from photogrammetric stereo compilation utilizing aerial photography at a scale of 1"= 700'
    Purpose: Cuyahoga Co. Landbase Mapping & LBRS Address Verification
  Time_Period_of_Content:
    Time_Period_Information:
      Range_of_Dates/Times:
        Beginning_Date: March 27, 2006
        Ending_Time: March 30, 2006
    Currentness_Reference: ground condition
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -81.764667
      East_Bounding_Coordinate: -81.599622
      North_Bounding_Coordinate: 41.530774
      South_Bounding_Coordinate: 41.474728
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: streams, lakes, rivers
      Theme_Keyword: Hydrography
  Access_Constraints: Access granted by County
  Use_Constraints: County needs notified of any and all use purpose
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Kevin Kelley
        Contact_Organization: Cuyahoga Co.
      Contact_Position: Engineer
  Browse_Graphic:
    Browse_Graphic_File_Name: HydroWest
    Browse_Graphic_File_Description: Approximate west half of Cuyahoga Co.
    Browse_Graphic_File_Type: .mdb
  Native_Data_Set_Environment: Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 2; ESRI ArcCatalog 9.2.0.1324
Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: String
      Point_and_Vector_Object_Count: 68548
Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: State Plane Coordinate System 1983
        State_Plane_Coordinate_System:
          SPCS_Zone_Identifier: 3401
          Lambert_Conformal_Conic:
            Standard_Parallel: 40.433333
            Standard_Parallel: 41.700000
            Longitude_of_Central_Meridian: -82.500000
            Latitude_of_Projection_Origin: 39.666667
            False_Easting: 1968500.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.001000
          Ordinate_Resolution: 0.001000
        Planar_Distance_Units: survey feet
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222
  Vertical_Coordinate_System_Definition:
    Altitude_System_Definition:
      Altitude_Resolution: 0.000001
      Altitude_Encoding_Method: Explicit elevation coordinate included with horizontal coordinates
Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Hydrography
    Attribute:
      Attribute_Label: igds_class
    Attribute:
      Attribute_Label: igds_style
    Attribute:
      Attribute_Label: igds_weight
    Attribute:
      Attribute_Label: igds_color
    Attribute:
      Attribute_Label: igds_graphic_group
    Attribute:
      Attribute_Label: igds_level
    Attribute:
      Attribute_Label: igds_level_name
    Attribute:
      Attribute_Label: elevation
    Attribute:
      Attribute_Label: SHAPE
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: OBJECTID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: SHAPE_Length
      Attribute_Definition: Length of feature in internal units.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Positive real numbers that are automatically generated.
    Attribute:
      Attribute_Label: Block
Distribution_Information:
  Resource_Description: Downloadable Data
Metadata_Reference_Information:
  Metadata_Date: 20071010
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: REQUIRED: The organization responsible for the metadata information.
        Contact_Person: REQUIRED: The person responsible for the metadata information.
      Contact_Address:
        Address_Type: REQUIRED: The mailing and/or physical address for the organization or individual.
        City: REQUIRED: The city of the address.
        State_or_Province: REQUIRED: The state or province of the address.
        Postal_Code: REQUIRED: The ZIP or other postal code of the address.
      Contact_Voice_Telephone: REQUIRED: The telephone number by which individuals can speak to the organization or individual.
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: http://www.esri.com/metadata/esriprof80.html
    Profile_Name: ESRI Metadata Profile
